Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VRRP Administration Guide

Search Scope:

- This Document
- Entire Library

#### Configuration Guidelines

Refer to the Sun Ethernet Fabric Operating System CLI Enterprise Reference Manual for a complete set of commands and options for configuring VRRP.

The command `vrrp vrid(1-255) ipv4 ip-address` must be entered for the current interface (with the correct `vrid`) before the execution of any commands in Interface Configuration mode.

This section shows the default configuration values:

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |