Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VLAN Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure Static Unicast Entry in Topology 2

For this procedure, you must first configure the VLAN. See Example Topolgy 2 for the topology for this procedure.

1. Configure the VLAN in switch 1.

       SEFOS# configure terminal
       SEFOS(config)# vlan 2
       SEFOS(config-vlan)# ports extreme-ethernet 0/3,0/15,0/19
       SEFOS(config-vlan)# exit
       SEFOS(config)# interface extreme-ethernet 0/15
       SEFOS(config-if)# no shutdown
       SEFOS(config-if)# exit
       SEFOS(config)# interface extreme-ethernet 0/19
       SEFOS(config-if)# no shutdown
       SEFOS(config-if)# exit
       SEFOS(config)# interface extreme-ethernet 0/3
       SEFOS(config-if)# no shutdown
       SEFOS(config-if)# exit
       SEFOS(config)# exit

2. Review the MAC address table.

       SEFOS# show mac-address-table
       Vlan      Mac Address           Type         Ports
       ---------------------------------------------------
       2         00:1b:21:53:6d:b9     Learnt       Ex0/19
       2         00:1b:21:53:6e:55     Static       Ex0/15
       2         01:02:03:04:05:06     Static       Ex0/3

       Total Mac Addresses Displayed: 3
       ------------------------------------------------

3. Review the created VLAN.

       SEFOS# show vlan id 2
       Vlan database
       -------------------
       Vlan ID             : 2
       Member Ports        : Ex0/3, Ex0/15, Ex0/19
       Untagged Ports      : None
       Forbidden Ports     : None
       Name                :
       Status              : Permanent
       ----------------------------------------------------

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |