Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the Report Suppression Interval

Reports sent to router ports can be suppressed for a specific period of time. You can configure the suppression time interval for which the IGMPv2 report messages for the same group are not forwarded onto the router ports. By default, the report suppression interval is 5 seconds. Before you can configure IGS features, you must configure your network environment, as described in Topology Example.

- Enable the Report Suppression Interval

- Disable the Report Suppression Interval

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |