Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Restore the Default Value of the OSPF Interface

A priority value of 0 signifies that the router is not eligible to become the designated router on a particular network. The default interface priority value is 1.

- Type.

      SEFOS(config-if)# no ip ospf priority

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |