Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure a Virtual Link

This example configures area `0.0.0.6` as a virtual link, with `20.0.0.1` as the virtual neighbor, and an interface index value of 100.

1. Enter Global Configuration mode in SEFOS1.

       SEFOS# configure terminal

2. Enable OSPF globally in SEFOS1.

       SEFOS(config)# ipv6 router ospf

3. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.0.0.1

4. Configure the virtual link.

       SEFOS(config-router)# area 0.0.0.6 virtual-link 20.0.0.1 100

5. View the configuration.

   Note - The neighbor state will be down until other end of the virtual link becomes active.

       SEFOS# show ipv6 ospf virtual-links

       Interface State: DOWN, Neighbor State: DOWN
       Transit Area: 0.0.0.6,  Virtual Neighbor: 20.0.0.1
       Intervals Configured for the Virtual Interface:
       Hello: 10, Dead: 60, Transit: 1, Retransmit : 5

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |