Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DHCP Administration Guide

Search Scope:

- This Document
- Entire Library

## Create an Excluded Address in the Pool

You can use this option to specify a range of IP addresses that cannot be allocated for the client. The `no` form of the command deletes the excluded pool.

In this example, the range of excluded address pools is `12.0.0.1` through `12.0.0.10`. The first available IP in this pool will be `12.0.0.11`.

1. Create the address pool.

       SEFOS# configure terminal
       SEFOS(config)# ip dhcp pool 1

2. Specify the excluded address pool.

       SEFOS(dhcp-config)# excluded-address 12.0.0.1 12.0.0.10
       SEFOS(dhcp-config)# end

3. View the excluded address pools.

       SEFOS# show ip dhcp server pools

   The output in switch 1 is:

       Pool Id                         : 1
       -------------------------------------------
       Subnet                          : 12.0.0.0
       Subnet Mask                     : 255.0.0.0
       Lease time                      : 95400 secs
       Utilization threshold           : 50%
       Start Ip                        : 12.0.0.1
       End Ip                          : 12.0.0.100
       Exclude Address Start IP        : 12.0.0.1
       Exclude Address End IP          : 12.0.0.10

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |