Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuration Parameters

This table contains the configuration parameters for the components in the example topology.

Node | Port | MAC Address | IP Address
--- | --- | --- | ---
Host A | eth0 | `00:11:22:33:44:0a` | `12.0.0.10`
Host B | eth0 | 00:11:22:33:44:0b | `12.0.0.20`
Host C | eth0 | 00:11:22:33:44:0c | `12.0.0.30`
SRC A | eth0 | 00:11:22:33:44:ee | `12.0.0.40`
SRC B | eth0 | 00:11:22:33:44:ff | `12.0.0.50`
DUT1 | P1 | `00:01:02:03:04:01` | `12.0.0.1`
P2 | `00:01:02:03:04:02`
P3 | `00:01:02:03:04:03`
P4 | `00:01:02:03:04:04`
P5 | `00:01:02:03:04:05`

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |