Skip Navigation Links
Exit Print View
| Oracle Ethernet Switches ### L2 and L3 Deployment Best Practices

Search Scope:

- This Document
- Entire Library

### Sun Network 10GbE Switch 72p

Sun Network 10GbE Switch 72p is a 1U standalone multipurpose TOR switch. The switch provides connection to external devices through 16 QSFP connectors with four 10GbE ports each and eight 10GbE SFP+ ports. The switch connects servers and storage devices in a rack environment.

For installation, configuration, and management information, refer to the documentation at: http://www.oracle.com/goto/SN-10GbE-72p/docs

##### Additional L2 and L3 Configurations for Sun Network 10GbE Switch 72p

For the following configurations, refer to the Sun Network 10GbE Switch 72p Software Configuration Guide at: http://www.oracle.com/goto/SN-10GbE-72p/docs

- Switching Feature

  - VLAN Forwarding

  - RSTP

  - LA

- Routing Feature

  - Static Unicast Route Entries

  - Dynamic Routing with RIP

  - Dynamic Routing with OSPF

##### Related Information

- Oracle Switch ES1-24

- Sun Blade 6000 Ethernet Switched NEM 24p 10GbE

Copyright © 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |