Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### SLB Administration Guide

Search Scope:

- This Document
- Entire Library

## Restart the Interface Following Failure

When the port 16 is repaired and recovered, use the following commands to ensure that the port status has returned to active.

1. Restart the interface.

       SEFOS# configure terminal
       SEFOS(config)# interface extreme-ethernet 0/16
       SEFOS(config-if)# no hutdown
       SEFOS(config-if)# end

2. After a few seconds, examine the SLB-L2 output.

       SEFOS# show slb l2

       L2 SLB Group #1
       Failover Method: Failover to All ports

       Members:
       Port   State     Comments
       ====   =====     =================
        15    ACTIVE
       16    ACTIVE
        17    ACTIVE
        18    ACTIVE

   Port 16 is now resumed to active state.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |