Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PVRST+ Administration Guide

Search Scope:

- This Document
- Entire Library

### Topology Example

This topology is referenced in the descriptions and instructions in this guide.

In this configuration, each switch A, B, and C, has two interfaces connected to the other two switches. Switch A has a third interface port 20 (P20) connected to a host. In addition to the default `VLAN 1`, `VLAN 10` and `VLAN 20` are used as command examples. The topology includes these details:

Switch | MAC Address | VLAN 10 Address and Mask
--- | --- | ---
A (hostname - NEM-1) | `00:14:4f:6c:56:6f` | `192.168.10.199`/`255.255.255.0`
B (hostname - TOR-1) | `00:14:4f:6c:69:ed` | `192.168.10.144`/`255.255.255.0`
C (hostname - TOR-2) | `00:14:4f:6c:6e:0d` | `192.168.10.149`/`255.255.255.0`

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |