Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LA Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the LACP Time-Out Value

The LACP time out value is a periodic interval. When the interval expires, an LACP PDU is sent out regularly. The default value for LACP time out is `long`. This list contains explanations of the possible values:

- `long` - The LACP PDU will be sent for every 30 seconds, and the LACP timeout value (when no packet is received from the peer) is 90 seconds.

- `short` - The LACP PDU will be sent every 1 second. The timeout value is 3 seconds.

1. Enter the configuration mode for the interface (0/1 in this example).

       SEFOS(config)# configure terminal
       SEFOS(config)# interface extreme-ethernet 0/1

2. Configure the LACP time out.

       SEFOS(config-if)# lacp timeout short

3. Review the `etherchannel` information.

       SEFOS# show etherchannel detail
       ...
       LACP Port Identifier = 1
       LACP Activity : Active
       LACP Timeout : Short
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |