Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DHCP Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable Traces for the DHCP Relay Agent

1. Enable DHCP relay debug traces in switch 2.

       SEFOS# debug ip dhcp relay all

2. View the debug trace level.

       SEFOS# show ip dhcp relay information

       Dhcp Relay                          : Enabled
       Default Circuit Id information        : router-index
       Dhcp Relay Servers only             : Enabled

       DHCP server                         : 20.0.0.1

       Dhcp Relay RAI option               : Enabled
       Default Circuit Id information        : router-index
       Debug Level                         : 0xff

       No of Packets inserted RAI option               : 0
       No of Packets inserted circuit ID suboption     : 0
       No of Packets inserted remote ID suboption      : 0
       No of Packets inserted subnet mask suboption    : 0
       No of Packets dropped                           : 0
       No of Packets which did not inserted RAI option : 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |