Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring RP Candidate Hold Time

Hold time is the amount of time the candidate RP advertisement is valid. Configure `rp-candidate holdtime` to set the hold time of the component when it is a candidate RP in the local domain.

- Specify RP Candidate Hold Time

- Restore the Default Candidate RP Hold Time

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |