Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Neighbor

This procedure specifies an NBMA neighbor router and its priority.

1. Type.

       SEFOS# configure terminal
       SEFOS(config)# router ospf

2. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.10.2.1

3. Configure the OSPF interface.

       SEFOS(config-router)# network 10.4.0.1 area 0.0.0.0
       SEFOS(config-router)# network 10.10.2.1 area 0.0.0.6

4. Exit Router Configuration mode.

       SEFOS(config)# exit

5. Enter Interface Configuration mode.

       SEFOS(config)# interface vlan 1

6. Configure the network type as NBMA.

       SEFOS(config-if)# ip ospf network non-broadcast

7. Configure the neighbor with priority.

       SEFOS(config-if)# exit
       SEFOS(config)# router ospf
       SEFOS(config-router)# neighbor 10.4.0.2 priority 10

8. Configure the neighbor with default priority.

       SEFOS(config-router)# no neighbor 10.4.0.2 priority 10

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |