Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring IPv6 Support in an Interface

IPv6 is the latest version of IP, which assigns a 128-bit IP address for the host and receiver. This IP address increases the address space and solves the IP address exhaustion caused by the IPv4 feature. To configure IPv6 support in an interface, you must enable IPv6 support in that interface.

These procedures show how to configure IPv6 support in an interface:

- Enable IPv6 Support

- Disable IPv6 Support

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |