Go to main content
oracle home
Sun Network 10GbE Switch 72p Product Notes

Exit Print View

Search Term
Search Scope:
This Document Entire Library
Updated: November 2016

- Sun Network 10GbE Switch 72p Product Notes
- Document Information
- Using This Documentation

- Product Documentation Library
- Feedback

- Late-Breaking Information

- Switch Documentation Reading Order
- New Features

- IPv6 Switching and Routing
- PVRST+ Protocol
- Exclusive VLAN
- Data Center Bridging
- Internet Group Management Protocol
- PIM
- Q-in-Q Tunneling
- Server Load Balancer Layer 3
- Uplink Port Trailing
- VRRPv3
- Oracle ILOM 3.0 Features

- Enhancements
- Upgrading the Switch Firmware

- Back Up the Current Configuration Before Upgrading
- Download the Switch Firmware Package
- Install the Switch Updates

- Configuring the Switch

- Configure 1Gbps Mode on SFP+ Interfaces
- Fine Tune the VLAN Setup
- Managing SEFOS Configurations

- Include the SEFOS Configuration in Backups
- Restore the Configuration

- Configuring TACACS+

- TACACS+ Properties
- Configure TACACS+ Settings

- Known Issues

- Manually Deleting Static Routes Does Not Affect the Corresponding SLB Entry (7123134)
- PIMv6-SSM Mode is Not Supported in This Release (7114280)
- Firmware Upgrade With the Web UI is Incomplete (7022295)
- Changing the Default Value for default-vlan-id Could Result in VLAN Misconfiguration (7015004)
- Some of the IGMP Conformance Results Do Not Match Expectations (7006297 and 6997415)
- QoS - set algo-type tailDrop queue-drop-algo Does Not Work (6991230)
- Packets Might Be Dropped When Using Q-in-Q Interop in Certain Configurations (6989048)
- The no default-metric [,short(1-16)>] Command Does Not Work as Documented (6987482)
- Using vlan 1 as Shown in Various Examples in the Documentation Generates Error Codes (6968484)
- When Multiple Configuration Scripts Are Run in Parallel, SEFOS Can Crash (6936742)
- The switch Command Line Option Is Unsupported
- vrrp_v3: Role is incorrect for vlan with no premempt configuration after save/reboot (19547263)
- SSL V3.0 POODLE DISABLE SSL V3 (19842635)
- Re-configure IP address after a "no ip address", previous config re-appears (18794861)

Language:

### Internet Group Management Protocol

The Internet Group Management Protocol (IGMP) (RFC 4604) implementation is used to learn and proxy the group membership information of the hosts connected to a router. Multicast routing protocols, like PIM, use this information to forward multicast packets that are received by the router. An IGMP proxy learns group membership and forwards multicast traffic based on this information. The proxy does not need to run any multicast routing protocols. IGMP proxy substitutes the information to upstream router interface, based on the requirements of IGMP hosts. This release of the firmware provides support for IGMP proxy.

Previous
Next