Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Test SEFOS9

SEFOS2 sends a type 7 LSA for the default route with the updated metric as 50. Therefore, the metric for the default route should be 51 in SEFOS9.

1. In SEFOS9, type.

       SEFOS# show ip ospf route

       OSPF Process Routing Table
       Dest/Mask                  TOS NextHop/Interface Cost Rt.Type   Area
       ---------                  --- -------/--------- ---- -------   ----
       0.0.0.0/0.0.0.0           0   10.2.2.2/vlan2    51   Type1Ext  0.0.0.2
       10.2.2.0/255.255.255.0    0   0.0.0.0/vlan2     1    IntraArea 0.0.0.2
       10.4.0.0/255.255.0.0      0   10.2.2.2/vlan2    2    InterArea 0.0.0.2

2. In SEFOS2, test the `no area default-cost` command.

       SEFOS# configure terminal
       SEFOS(config)# router ospf
       SEFOS(config-router)# no area 0.0.0.2 default-cost

3. In SEFOS9, type.

       SEFOS# show ip ospf route

       OSPF Process Routing Table
       Dest/Mask                     TOS NextHop/Interface Cost Rt.Type   Area
       ---------                     --- -------/--------- ---- -------   ----
       0.0.0.0/0.0.0.0               0   10.2.2.2/vlan2    11    Type1Ext 0.0.0.2
       10.2.2.0/255.255.255.0        0   0.0.0.0/vlan2     1    IntraArea 0.0.0.2
       10.4.0.0/255.255.0.0          0   10.2.2.2/vlan2    2    InterArea 0.0.0.2

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |