Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Static RPs

Static configuration allows additional structuring of the multicast traffic by directing the multicast JP messages to statically configured RPs. Configure `rp-static rp-address` to set the address for the interface that will be advertised as a static RP.

- Specify the Address for the Static RP

- Delete a Static RP

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |