Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Test the Summary Address Configuration

1. On switch 1, configure the `summary-address` option.

       SEFOS# configure terminal
       SEFOS(config)# router rip
       SEFOS(config-router)# network 10.0.0.1
       SEFOS(config-router)# redistribute all

2. Disable the `auto-summary` option.

       SEFOS(config-router)# auto-summary disable
       SEFOS(config-router)# exit

3. Configure the static routes.

       SEFOS(config-router)# ip route 40.1.0.0 255.255.0.0 vlan 2
       SEFOS(config-router)# ip route 40.2.0.0 255.255.0.0 vlan 2
       SEFOS(config-router)# ip route 40.3.0.0 255.255.0.0 vlan 2
       SEFOS(config-router)# ip route 40.4.0.0 255.255.0.0 vlan 2

4. Configure the summary address for the `VLAN 1` interface (`20.0.0.0/8`).

       SEFOS(config)# interface vlan 1
       SEFOS(config-if)# ip rip summary-address 40.0.0.0 255.0.0.0
       SEFOS(config-if)# end

5. On switch 2, configure the interface for `VLAN 1`.

       SEFOS# configure terminal
       SEFOS(config)# router rip
       SEFOS(config-router)# network 10.0.0.2
       SEFOS(config-router)# end

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |