Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable the General Query Transmission Option

1. Enter Global Configuration mode.

       SEFOS# configure terminal

2. Enable the transmission of the IGMP general query for any topology change.

       SEFOS(config)# ip igmp snooping send-query enable
       SEFOS(config)# end

3. Review the configuration.

       SEFOS# show ip igmp snooping globals

       Snooping Configuration
         -----------------------------
         IGMP Snooping globally enabled
         IGMP Snooping is operationally enabled
         IGMP Snooping Enhanced mode is disabled
         Transmit Query on Topology Change globally enabled
         Multicast forwarding mode is MAC based
         Proxy globally disabled
         Proxy reporting globally enabled
         Filter is disabled
         Router port purge interval is 125 seconds
         Port purge interval is 260 seconds
         Report forward interval is 5 seconds
         Group specific query interval is 2 seconds
         Reports are forwarded on router ports
         Group specific query retry count is 2
         Multicast VLAN disabled
         Leave config level is Vlan based

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |