Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure Switch 1

Use the following commands to configure `VLAN 1` and `VLAN 2` on switch 1 in the example topologies.

- Configure switch 1.

      SEFOS# configure terminal
      SEFOS(config)# set gvrp disable
      SEFOS(config)# set gmrp disable
      SEFOS(config)# interface vlan 1
      SEFOS(config-if)# shutdown
      SEFOS(config-if)# ip address 10.0.0.1 255.255.0.0
      SEFOS(config-if)# no shutdown
      SEFOS(config-if)# exit
      SEFOS(config)# vlan 1
      SEFOS(config-vlan)# ports extreme-ethernet 0/1 untagged extreme-ethernet 0/1
      SEFOS(config-vlan)# exit
      SEFOS(config)# interface vlan 2
      SEFOS(config-if)# shutdown
      SEFOS(config-if)# ip address 20.2.2.2 255.255.255.0
      SEFOS(config-if)# no shutdown
      SEFOS(config-if)# exit
      SEFOS(config)# vlan 2
      SEFOS(config-vlan)# ports extreme-ethernet 0/2 untagged extreme-ethernet 0/2
      SEFOS(config-vlan)# exit
      SEFOS(config)# interface extreme-ethernet 0/2
      SEFOS(config-if)# switchport pvid 2

      SEFOS(config-if)# no shutdown
      SEFOS(config-if)# exit

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |