Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable MLDS in a Specific VLAN

When MLDS is enabled globally, it is enabled in all the existing VLAN interfaces. When MLD snooping is disabled globally, it is disabled in all the existing VLAN interfaces. However, you can enable MLDS on specific VLANs, as described in the following example.

In this example, MLDS is enabled on `VLAN 2`.

1. Specify the VLAN for which MLDS is to be enabled.

       SEFOS# configure terminal
       SEFOS(config)# vlan 2

2. Enable MLDS on the specified VLAN.

       SEFOS(config-vlan)# ipv6 mld snooping
       SEFOS(config-vlan)# end

3. View the configuration.

       SEFOS# show ipv6 mld snooping vlan 2

       Snooping VLAN Configuration for the VLAN 2
         MLD Snooping enabled
         MLD Operating version is V2
         Fast leave is disabled
         Snooping switch is acting as Non-Querier
         Query interval is 125 seconds

   When MLDS is globally enabled or disabled, but not enabled on `VLAN 2`, the second line in the output of this command is:

       MLD Snooping disabled

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |