Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the regstop Rate Limit

A register-stop message avoids the encapsulation of multicast data packets from the first-hop router to the RP. Configuring the `regstop` rate limit specifies the time interval between two successive register-stop messages sent by an RP.

1. Enable PIMv6.

       SEFOS# configure terminal
       SEFOS(config)# set ipv6 pim enable

2. Set the regstop rate limit value to 10 seconds.

       SEFOS(config)# set ip pim regstop-ratelimit-period 10
       SEFOS(config)# end

3. Review the regstop rate limit value.

       SEFOS# show ipv6 pim thresholds

       PIM SPT Threshold Information
       -----------------------------
         Group Threshold  : 0
         Source Threshold : 0
         Switching Period : 0
       PIM SPT-RP Threshold Information
       --------------------------------
         Register Threshold       : 10
         RP Switching Period      : 15
         Register Stop rate limit : 10

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |