Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the Port-Purge Interval

The expiration of the port-purge timer on the port for a particular multicast group results in the port being removed from the forwarding list of the corresponding multicast entry in the multicast forwarding table. Before you can configure IGS features, you must configure your network environment, as described in Topology Example.

- Set the Port-Purge Interval

- Reset the Port-Purge Interval

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |