Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DHCP Administration Guide

Search Scope:

- This Document
- Entire Library

## Protocol Description

DHCP enables dynamic configuration of a host computer. When a DHCP client is turned on, it issues a broadcast message to any DHCP server that is on the network. An exchange takes place during which the DHCP server assigns an IP address to the client and informs the client of certain key network configuration parameters.

The SEFOS DHCP implementation complies with RFC 2131.

- DHCP Server

- DHCP Client

- DHCP Relay Agent

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |