Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### SLB Administration Guide

Search Scope:

- This Document
- Entire Library

#### SLB Configuration Guidelines and Prerequisites

These guidelines and prerequisites apply to SLB configurations:

- Set up as many as 16 servers per SLB group.

- Establish up to 16 SLB groups.

- Set up as many as 32 servers on the switch for load balancing.

- Ensure that server members within an SLB group do not span multiple VLANs.

- Choose any IP address for a VIP, ensuring that the IP address is not in the same subnet as the physical server’s subnet.

- Although it is not a strict requirement, you should disable switch ports that are involved in the SLB before setting up SLB.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |