Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIPng Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable and Configure RIPng on Desired IPv6 Interfaces

1. Enable RIPng on the interfaces on SEFOS1.

       SEFOS 1 SEFOS# configure terminal
       SEFOS 1 SEFOS(config)# interface vlan 30
       SEFOS 1 SEFOS(config-if)# ipv6 rip enable
       SEFOS 1 SEFOS(config-if)# exit

       SEFOS 1 SEFOS(config)# interface vlan 40
       SEFOS 1 SEFOS(config-if)# ipv6 rip enable
       SEFOS 1 SEFOS(config-if)# exit

       SEFOS 1 SEFOS(config)# interface vlan 50
       SEFOS 1 SEFOS(config-if)# ipv6 rip enable
       SEFOS 1 SEFOS(config-if)#

2. Enable RIPng on the interfaces on SEFOS2.

       SEFOS 2 SEFOS# configure terminal
       SEFOS 2 SEFOS(config)# interface vlan 10
       SEFOS 2 SEFOS(config-if)# ipv6 rip enable
       SEFOS 2 SEFOS(config-if)# exit

       SEFOS 2 SEFOS(config)# interface vlan 40
       SEFOS 2 SEFOS(config-if)# ipv6 rip enable
       SEFOS 2 SEFOS(config-if)# exit

3. Enable RIPng on the interfaces on SEFOS3.

       SEFOS 3 SEFOS# configure terminal
       SEFOS 3 SEFOS(config)# interface vlan 20
       SEFOS 3 SEFOS(config-if)# ipv6 rip enable
       SEFOS 3 SEFOS(config-if)# exit

       SEFOS 3 SEFOS(config)# interface vlan 30
       SEFOS 3 SEFOS(config-if)# ipv6 rip enable
         SEFOS 3 SEFOS(config-if)# exit

4. Review the RIPng status on SEFOS1.

       SEFOS 1 SEFOS# show ipv6 rip
       RIP  port 521, multicast-group ff02::9,Maximum paths is 16
       Updates every 30 seconds; expire after 180SEFOS 1 SEFOS# show ipv6 rip  database
       Garbage Collect after  120 secondsRIP local RIB 1111::/112,  metric 2, ripng      vlan40/fe80::214:4fff:fe6c:630f, expires in 180 secs 2222::/112,  metric 2, ripng      vlan30/fe80::214:4fff:fe6c:686d, expires in 180 secs 3333::/112,  metric 2, ripng      vlan30/fe80::214:4fff:fe6c:686d, expires in 180 secs 3333::/112,  metric 1, local      vlan30/::, expires in 180 secs 4444::/112,  metric 2, ripng      vlan40/fe80::214:4fff:fe6c:630f, expires in 180 secs 4444::/112,  metric 1, local      vlan40/::, expires in 180 secs 5555::/112,  metric 1, local      vlan50/::, expires in 180 secs 6666::/112,  metric 2, ripng      vlan40/fe80::214:4fff:fe6c:630f, expires in 180 secs
       Poison Reverse is on
       Interface:
       vlan50
       vlan40
       vlan30
       Redistribution:
       Connected,Routes  Redistribution is enabled.

       SEFOS 1 SEFOS# show ipv6 route
       IPv6 Routing Table  -  8 entries
       Codes : C - Connected, S - StaticSEFOS 1 SEFOS# show ipv6 route summary
       O - OSPF, R - RIP, B - BGPIPv6 Routing Table Summary - 8 entries    3 Connected, 0 Static, 5 RIP, 0 BGP, 0 OSPF        Number of prefixes:    /112: 8
       R   1111::/112   [2/120]
       via fe80::214:4fff:fe6c:630f, vlan40
       R   2222::/112   [2/120]
       via fe80::214:4fff:fe6c:686d, vlan30
       C   3333::/112   [1/1]
       via ::, vlan30
       R   3333::/112   [2/120]
       via fe80::214:4fff:fe6c:686d, vlan30
       C   4444::/112   [1/1]
       via ::, vlan40
       R   4444::/112   [2/120]
       via fe80::214:4fff:fe6c:630f, vlan40
       C   5555::/112   [1/1]
       via ::, vlan50
       R   6666::/112   [2/120]
       via fe80::214:4fff:fe6c:630f, vlan40

5. Review the RIP route on SEFOS2.

       SEFOS 2 SEFOS# show ipv6 rip
       RIP  port 521, multicast-group ff02::9,Maximum paths is 16
       Updates every 30 seconds; expire after 180SEFOS 2 SEFOS# show ipv6 rip  database
       Garbage Collect after  120 secondsRIP local RIB 1111::/112,  metric 1, local      vlan10/::, expires in 180 secs 2222::/112,  metric 3, ripng      vlan40/fe80::221:28ff:fe56:d7a9, expires in 180 secs 3333::/112,  metric 2, ripng      vlan40/fe80::221:28ff:fe56:d7a9, expires in 180 secs 4444::/112,  metric 1, local      vlan40/::, expires in 180 secs 5555::/112,  metric 2, ripng      vlan40/fe80::221:28ff:fe56:d7a9, expires in 180 secs 6666::/112,  metric 1, local      vlan10/::, expires in 180 secs
       Poison Reverse is on
       Interface:
       vlan40
       vlan10
       Redistribution:
       Connected,Routes  Redistribution is enabled.

       SEFOS 2 SEFOS# show ipv6 route
       IPv6 Routing Table  -  6 entries
       Codes : C - Connected, S - StaticSEFOS 2 SEFOS# show ipv6 route summary
       O - OSPF, R - RIP, B - BGPIPv6 Routing Table Summary - 6 entries    3 Connected, 0 Static, 3 RIP, 0 BGP, 0 OSPF        Number of prefixes:    /112: 6
       C   1111::/112   [1/1]
       via ::, vlan10
       R   2222::/112   [3/120]
       via fe80::221:28ff:fe56:d7a9, vlan40
       R   3333::/112   [2/120]
       via fe80::221:28ff:fe56:d7a9, vlan40
       C   4444::/112   [1/1]
       via ::, vlan40
       R   5555::/112   [2/120]
       via fe80::221:28ff:fe56:d7a9, vlan40
       C   6666::/112   [1/1]
       via ::, vlan10

6. Review the RIP route on SEFOS3.

       SEFOS 3 SEFOS# show ipv6 rip
       RIP  port 521, multicast-group ff02::9,Maximum paths is 16
       Updates every 30 seconds; expire after 180SEFOS 3 SEFOS# show ipv6 rip  database
       Garbage Collect after  120 secondsRIP local RIB 1111::/112,  metric 3, ripng      vlan30/fe80::221:28ff:fe56:d7a9, expires in 180 secs 2222::/112,  metric 1, local      vlan20/::, expires in 180 secs 3333::/112,  metric 2, ripng      vlan30/fe80::221:28ff:fe56:d7a9, expires in 180 secs 3333::/112,  metric 1, local      vlan30/::, expires in 180 secs 4444::/112,  metric 2, ripng      vlan30/fe80::221:28ff:fe56:d7a9, expires in 180 secs 5555::/112,  metric 2, ripng      vlan30/fe80::221:28ff:fe56:d7a9, expires in 180 secs 6666::/112,  metric 3, ripng      vlan30/fe80::221:28ff:fe56:d7a9, expires in 180 secs
       Poison Reverse is on
       Interface:
       vlan20
       vlan30
       Redistribution:
       Connected,Routes  Redistribution is enabled.

       SEFOS 3 SEFOS# show ipv6 route
       IPv6 Routing Table  -  7 entries
       Codes : C - Connected, S - StaticSEFOS 3 SEFOS# show ipv6 route summary
       O - OSPF, R - RIP, B - BGPIPv6 Routing Table Summary - 7 entries    2 Connected, 0 Static, 5 RIP, 0 BGP, 0 OSPF        Number of prefixes:    /112: 7
       R   1111::/112   [3/120]
       via fe80::221:28ff:fe56:d7a9, vlan30
       C   2222::/112   [1/1]
       via ::, vlan20
       C   3333::/112   [1/1]
       via ::, vlan30
       R   3333::/112   [2/120]
       via fe80::221:28ff:fe56:d7a9, vlan30
       R   4444::/112   [2/120]
       via fe80::221:28ff:fe56:d7a9, vlan30
       R   5555::/112   [2/120]
       via fe80::221:28ff:fe56:d7a9, vlan30
       R   6666::/112   [3/120]
       via fe80::221:28ff:fe56:d7a9, vlan30

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |