Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring a Passive Interface

You can configure a passive interface to suppress routing updates on all interfaces or specified interfaces. If you configure a passive interface for all interfaces, all OSPF interfaces will be passive. This situation is useful in ISP environments and for large enterprise networks, where many of the distribution routers have more than 200 interfaces.

- Configure All Interfaces To Be Passive

- Configure Specified Interfaces To Be Passive

- Restore the Default Routing Updates

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |