Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

#### SFP+ Cables

The SFP+ connectors support the following types of cables:

- 10 Gbyte/1 Gbyte dual speed fiber

- 1 Gbyte RJ-45 copper

- 10 Gbps direct attach copper

The active fiber SFP+ Ethernet cable is a dual-part unit, where the cable and the optical tranceiver are separate parts.

The SFP+ Ethernet cables are single-part (cable and transceiver combined) and dual-part (cable and transceiver separate) units.

The active fiber SFP+ Ethernet cable is a dual-part unit, where the cable and the optical tranceiver are separate parts.

The passive copper Ethernet cable is a single-part unit, where the cable and the tranceiver (cable connector) are a single combined assembly.

##### Related Information

- Install the Switch in the Rack

- Splitter Cables

- QSFP Cables

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |