Go to main content
oracle home
Sun Network 10GbE Switch 72p Product Notes

Exit Print View

Search Term
Search Scope:
This Document Entire Library
Updated: November 2016

- Sun Network 10GbE Switch 72p Product Notes
- Document Information
- Using This Documentation

- Product Documentation Library
- Feedback

- Late-Breaking Information

- Switch Documentation Reading Order
- New Features

- IPv6 Switching and Routing
- PVRST+ Protocol
- Exclusive VLAN
- Data Center Bridging
- Internet Group Management Protocol
- PIM
- Q-in-Q Tunneling
- Server Load Balancer Layer 3
- Uplink Port Trailing
- VRRPv3
- Oracle ILOM 3.0 Features

- Enhancements
- Upgrading the Switch Firmware

- Back Up the Current Configuration Before Upgrading
- Download the Switch Firmware Package
- Install the Switch Updates

- Configuring the Switch

- Configure 1Gbps Mode on SFP+ Interfaces
- Fine Tune the VLAN Setup
- Managing SEFOS Configurations

- Include the SEFOS Configuration in Backups
- Restore the Configuration

- Configuring TACACS+

- TACACS+ Properties
- Configure TACACS+ Settings

- Known Issues

- Manually Deleting Static Routes Does Not Affect the Corresponding SLB Entry (7123134)
- PIMv6-SSM Mode is Not Supported in This Release (7114280)
- Firmware Upgrade With the Web UI is Incomplete (7022295)
- Changing the Default Value for default-vlan-id Could Result in VLAN Misconfiguration (7015004)
- Some of the IGMP Conformance Results Do Not Match Expectations (7006297 and 6997415)
- QoS - set algo-type tailDrop queue-drop-algo Does Not Work (6991230)
- Packets Might Be Dropped When Using Q-in-Q Interop in Certain Configurations (6989048)
- The no default-metric [,short(1-16)>] Command Does Not Work as Documented (6987482)
- Using vlan 1 as Shown in Various Examples in the Documentation Generates Error Codes (6968484)
- When Multiple Configuration Scripts Are Run in Parallel, SEFOS Can Crash (6936742)
- The switch Command Line Option Is Unsupported
- vrrp_v3: Role is incorrect for vlan with no premempt configuration after save/reboot (19547263)
- SSL V3.0 POODLE DISABLE SSL V3 (19842635)
- Re-configure IP address after a "no ip address", previous config re-appears (18794861)

Language:

## Using This Documentation

- Overview – Contains late-breaking information about this release of Oracle's Sun Network 10GbE Switch 72p

- Audience – Technicians, system administrators, authorized service providers, and advanced users

- Required knowledge – Advanced experience troubleshooting and replacing hardware

### Product Documentation Library

Documentation and resources for this product and related products are available at http://docs.oracle.com/cd/E19934-01/index.html.

### Feedback

Provide feedback about this documentation at http://www.oracle.com/goto/docfeedback.

Previous
Next