Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PVRST+ Administration Guide

Search Scope:

- This Document
- Entire Library

## Set Up PVID on a Port

1. Enter the configuration mode for the interface.

       TOR-1 SEFOS# configure terminal
       TOR-1 SEFOS(config)# interface  extreme-ethernet 0/1
       TOR-1 SEFOS(config-if)#

2. Set the PVID value.

       TOR-1 SEFOS(config-if)# switchport pvid 10
       TOR-1 SEFOS(config-if)# end
       TOR-1 SEFOS#

3. Display VLAN related parameters for port 0/1.

       TOR-1 SEFOS# show vlan port config port extreme-ethernet 0/1

       Vlan Port configuration table
       -------------------------------
       Port Ex0/1
        Port Vlan ID                     : 10
        Port Acceptable Frame Type       : Admit Only Untagged and Priority Tagged
        Port Ingress Filtering           : Disabled
        Port Mode                        : Access
        Port Gvrp Status                 : Disabled
        Port Gmrp Status                 : Enabled
        Port Gvrp Failed Registrations   : 0
        Gvrp last pdu origin                : 00:00:00:00:00:00
        Port Restricted Vlan Registration   : Disabled
        Port Restricted Group Registration  : Disabled
        Mac Based Support                   : Disabled
        Subnet Based Support                : Disabled
        Port-and-Protocol Based Support     : Enabled
        Default Priority                    : 0
        Filtering Utility Criteria          : Default
        Port Protected Status               : Disabled
        -------------------------------------------------------

       TOR-1 SEFOS#

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |