Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Report Forwarding

By default, when an MLD report is received, it is forwarded to all router ports. However, it is also possible to configure the received reports to be forwarded on the member ports of the VLAN. In addition, you can suppress the sending of reports to router ports for a specified period of time. During the amount of time you specify, MLD report messages for the same group will not get forwarded onto the router ports.

- Forward MLD Reports to All Ports

- Forward MLD Reports Only to Router Ports

- Restore the Default MLD Report-Forwarding Status

- Configure the Report Forward Suppression Interval

- Restore the Default Report Forward Suppression Interval

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |