Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### SLB Administration Guide

Search Scope:

- This Document
- Entire Library

#### Separate VLAN SLB Configuration

The following figure illustrates an SLB configuration with servers and clients on separate VLANs. Servers are directly connected to the switch.

Feature | Default Settings
--- | ---
VIP | `10.10.10.1`
Active servers’ RIP | `192.0.0.1`, `192.0.0.2`, `192.0.0.3`
Standby servers’ RIP | `192.0.0.4`
Client subnet, VLAN 2 | `20.0.0.0`/`24`
Client subnet interface address | `20.0.0.100`
Server subnet, VLAN 3 | `192.0.0.0`/`24`
Server subnet interface address | `192.0.0.100`
Switch ports used by servers | Extreme-ethernet 0/15-18
Switch ports used by client network | Extreme-ethernet 0/3-6
Network interface for both servers | `ixgbe0`

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |