Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the NSSA Area Translation Role

This procedure configures the translation role for the NSSA as always or candidate.

1. Type.

       SEFOS# configure terminal
       SEFOS(config)# router ospf

2. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.10.2.1

3. Configure the ASBR router status.

       SEFOS(config-router)# asbr router

4. Configure the OSPF interface.

       SEFOS(config-router)# network 10.10.2.1 area 0.0.0.6

5. Configure the area `0.0.0.6` as an NSSA area.

       SEFOS(config-router)# area 0.0.0.6 nssa

6. Configure the translation role for the NSSA area `0.0.0.6`.

       SEFOS(config-router)# area 0.0.0.6 translation-role always

7. Configure the default translation role for the NSSA area `0.0.0.6`.

       SEFOS(config-router)# no area 0.0.0.6 translation-role

   Note - The default translation role is candidate. Configure the default translation role with the `no area area-id translation-role` command.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |