Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Test the Host

This example tests whether an intra-area-prefix-LSA carries the host entries.

- Test the host, SEFOS10.

      SEFOS# show ipv6 ospf database intra-prefix detail

      Age: 0   Seconds            LS Type: Intra Area Prefix Lsa
      Link State Id: 0.0.0.0      Adv Rtr Id: 11.0.0.1
      Sequence: 0x80000004        Checksum: 0xe526    Length: 52
      #Prefixes: 1                Referenced LS Type: Router Lsa
      Ref Link State Id: 0.0.0.0   Ref Adv Router: 11.0.0.1
      Prefix Length (Bytes): 16    Prefix Options: 0x00
      Metric: 0xa
      Prefix: fec0::3556:1:1

      Age: 0   Seconds            LS Type: Intra Area Prefix Lsa
      Link State Id: 0.0.0.1      Adv Rtr Id: 11.0.0.1
      Sequence: 0x80000001        Checksum: 0x5cbe    Length: 48
      #Prefixes: 1                Referenced LS Type: Network Lsa
      Ref Link State Id: 0.0.0.34  Ref Adv Router: 11.0.0.1
      Prefix Length (Bytes): 12    Prefix Options: 0x00
      Metric: 0x0
      Prefix: fec0::3556:0:0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |