Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

### Default Settings

This table shows the default values configured in the router when PIMv6 is enabled. These default values can be changed at any time.

Feature | Default Value
--- | ---
Module status | Disable
SPT group threshold | 0
SPT source threshold | 0
SPT switch period | 0 second
RP threshold | 0
RP switch period | 0 second
`regstop` rate limit period | 5 seconds
PMBR status | Disabled
Static RP | Disabled
Component mode | Sparse
RP-candidate hold time | 0 second
Query interval | 30 seconds
Message interval | 60 seconds
BSR candidate | 0
Component ID | 1
Hello hold time | 105 seconds
DR priority | 1
Override interval | 0 second
LAN delay | 0 second
LAN-prune delay | Disable

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |