Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

## Disable LAN Prune Delay

LAN prune delay is disabled by default. If you have previously enabled LAN prune delay and want to disable it, complete these steps.

- Disable LAN prune delay.

      SEFOS# configure terminal
      SEFOS(config)# interface vlan 5
      SEFOS(config)# set ip pim lan-prune-delay disable
      SEFOS(config)# end

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |