Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Spanning Tree L2GP Status

To configure a port as L2GP, you must disable the BPDU transmit status.

1. Disable the BPDU transmit status.

       SEFOS# configure terminal
       SEFOS(config)# interface extreme-ethernet 0/1

   Valid interfaces include physical interfaces and `port-channel` logical interfaces (`port-channel` port-channel-number).

       SEFOS(config)# spanning-tree bpdu-transmit disabled

2. Configure the port as L2GP.

       SEFOS(config)# spanning-tree layer2-gateway-port

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |