Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Stub Area

Configuring the stub area specifies an area as a stub area. This procedure also configures other parameters related to that area. See Stub Area, ASBR, and Route Redistribution Topology Example for the topology for this procedure.

1. Type.

       SEFOS# configure terminal
       SEFOS(config)# router ospf
       SEFOS(config-router)# router-id 10.10.2.1
       SEFOS(config-router)# network 10.4.0.1 area 0.0.0.0
       SEFOS(config-router)# network 10.10.2.1 area 0.0.0.6

2. Configure the area `0.0.0.6` as a normal area.

       SEFOS(config-router)# area 0.0.0.6 stub

3. Reconfigure the area `0.0.0.6` as a normal area.

       SEFOS(config-router)# no area 0.0.0.6 stub

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |