Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LLDP Administration Guide

Search Scope:

- This Document
- Entire Library

## Clear the LLDP Remote Table

LLDP remote table is updated whenever LLDP operates in the transmit and receive-receive only modes.

1. At both switches, configure the LLDP module status as enabled.

   See Configure the LLDP Module Status.

2. On both switches, enter the Global Configuration mode.

       SEFOS# configure terminal

3. Allow both switches to learn the neighbors, then clear the LLDP remote table.

       SEFOS(config)# clear lldp table
       SEFOS(config)# end

4. On both switches, review the remote table.

       SEFOS# show lldp neighbors
       Capability Codes        :
       (R) Router, (B) Bridge, (T) Telephone, (C) DOCSIS Cable Device,
       (W) WLAN Access Point, (P) Repeater, (S) Station, (O) Other

       Chassis ID        Local Intf        Hold-time    Capability    Port Id
       ----------        ----------        ---------    ----------    -------
       Total Entries Displayed    : 0

Copyright © 2010, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |