Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the P-bit Setting in the Default Type 7 LSA

This procedure enables the setting of the P-bit in the default Type 7 LSA generated by the NSSA internal ASBR.

1. Type.

       SEFOS# configure terminal
       SEFOS(config)# router ospf

2. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.10.2.1

3. Configure the ASBR router status.

       SEFOS(config-router)# asbr router

4. Configure the OSPF interface.

       SEFOS(config-router)# network 10.10.2.1 area 0.0.0.6

5. Configure the area `0.0.0.6` as an NSSA area.

       SEFOS(config-router)# area 0.0.0.6 nssa

6. Enable nssa asbr-default-route translator.

       SEFOS(config-router)# set nssa asbr-default-route translator enable

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |