Skip Navigation Links
Exit Print View
| Oracle Ethernet Switches ### L2 and L3 Deployment Best Practices

Search Scope:

- This Document
- Entire Library

## Prepare Switch `ToR72p-1` for L2 PVRST Active/Standby on the Servers

Note - The procedure for configuring `ToR72p-1` for L2 PVRST Active/Standby and standard L2 PVRST is the same.

- Perform the steps for configuring `ToR72p-1` for standard L2 PVRST.

  Go to Configure Switch `ToR72p-1` for L2 PVRST.

##### Related Information

- Prepare Switch `ToR72p-2` for L2 PVRST Active/Standby on the Servers

- Configure Switch `ES1-24p-1` for L2 PVRST Active/Standby on the Servers

- Configure Switch `ES1-24p-2` for L2 PVRST Active/Standby on the Servers

- Verify the L2 PVRST Active/Standby Configuration on the Servers

Copyright © 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |