Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Group and Source Thresholds

Configuring the PIMv6 group threshold sets the maximum limit for the rate of the flow of data in the group. Configuring the source threshold sets the maximum limit for the rate of the flow of data from the source to the receiver. When the rate of the flow of data exceeds the SPT group or source threshold, switching to the SPT is initiated. You must configure the threshold value to switch to SPT.

1. Enable PIMv6 in the router.

       SEFOS# configure terminal
       SEFOS(config)# set ipv6 pim enable
       SEFOS(config)# end

2. Set the SPT group threshold to 10 data packets.

       SEFOS# configure terminal
       SEFOS(config)# set ip pim threshold spt-grp 10

3. Set the SPT source threshold to 15 data packets.

       SEFOS(config)# set ip pim threshold spt-src 15
       SEFOS(config)# end

4. Review the threshold values.

       SEFOS# show ipv6 pim thresholds

       PIM SPT Threshold Information
       -----------------------------
         Group Threshold  : 10
         Source Threshold : 15
         Switching Period : 0

       PIM SPT-RP Threshold Information
       --------------------------------
         Register Threshold       : 0
         RP Switching Period      : 0
         Register Stop rate limit : 5

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |