Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Remove IPv6 Addresses From an Interface

1. Enter Interface Configuration mode for the `VLAN 1` interface.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 1

2. Delete the IPv6 address configured for that interface.

       SEFOS(config-if)# no ipv6 address fec0::1111:0:1 96
       SEFOS(config-if)# no ipv6 address fe80::203:2ff:fe03:501 link-local
       SEFOS(config-if)# exit
       SEFOS(config)# exit

3. Review the IPv6 information for the `VLAN 1` interface.

       SEFOS# show ipv6 interface vlan 1

       vlan1 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::214:4fff:fe6c:560f
       ...

   The link-local address is auto-configured when you remove a link-local address in the IPv6 interface.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |