Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Generation of a Default External Route

This procedure enables the generation of a default external route into the OSPF routing domain and other parameters related to that area. See Generation of a Default External Route and Redistribution Configuration Topology Example for the topology for this procedure.

1. Type.

       SEFOS# configure terminal
       SEFOS(config)# router ospf

2. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.10.2.1

3. Enable OSPF over the VLAN interface and associate the interface with an OSPF area.

       SEFOS(config-router)# network 10.4.0.1 area 0.0.0.0
       SEFOS(config-router)# network 10.10.2.1 area 0.0.0.6

4. Configure the ASBR router status.

       SEFOS(config-router)# asbr outer

5. Configure the generation of a default external route.

       SEFOS(config-router)# default-information originate always metric 40

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |