Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure SEFOS1

1. Disable generation of a default external route.

       SEFOS# configure terminal
       SEFOS(config)# router ospf
       SEFOS(config-router)# no default-information originate always
       SEFOS(config-router)# end
       SEFOS#

2. Examine the results.

   Type 5 External LSA for the default route must be flushed.

       SEFOS# show ip ospf database external

       OSPF Router with ID (10.10.2.1)

3. In SEFOS2, observe that the route entry for the default route has been deleted.

       SEFOS# show ip ospf route

       OSPF Process Routing Table
       Dest/Mask                  TOS NextHop/Interface Cost Rt.Type   Area
       ---------                     --- -------/--------- ---- -------   ----
       10.2.2.0/255.255.255.0     0   0.0.0.0/vlan2     1    IntraArea 0.0.0.2
       10.4.0.0/255.255.0.0       0   0.0.0.0/vlan1     1    IntraArea 0.0.0.0
       10.10.0.0/255.255.0.0      0   10.4.0.1/vlan1    2    InterArea 0.0.0.0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |