Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System Uplink Port Trailing Administration Guide

Search Scope:

- This Document
- Entire Library

### Uplink Port Trailing Topology Example

The following topology demonstrates the Uplink Port Trailing feature configured on access switches connecting to the servers. The example uses the Sun Blade 6000 Ethernet Switched NEM 24p 10GbE at the access layer. To enable this feature, the interfaces connecting from the access switch to the Sun Ethernet 10GbE Switch 72 (ToR72) and server-facing interfaces are bound together in a group.

Copyright © 2015, Oracle and/or its affiliates. All rights reserved. Legal Notices |