Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Bridge Priority

When setting the bridge priority, you can specify a value of 0 to 61440, in increments of 4096. Valid priority values are 0, 4096, 8192, 12288, 16384, 20480, 24576, 28672, 32768, 36864, 40960, 45056, 49152, 53248, 57344, and 61440. All other values are rejected. The default value is 32768. The lower the number, the more likely the switch is chosen as the root switch.

- Configure the Bridge Priority

- Restore the Default Bridge Priority

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |