Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Convert a Stub Area to a Normal Area

You can convert an area previously identified as a stub area to a normal area.

This example reconfigures area `0.0.0.6` as a normal area.

- Return a stub area to a normal area.

      SEFOS(config-router)# no area 0.0.0.6 stub

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |