Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### SLB Administration Guide

Search Scope:

- This Document
- Entire Library

## Set Up the Client

1. Set up the clients’ network interfaces if they are not already set up.
2. Establish a route entry to the VIP.

       client1% route add 10.10.10.1/24 20.0.0.100

   In this example, all client initiated traffic with a destination IP address of `10.10.10.1` will be forwarded to the gateway interface `20.0.0.100`.

3. If the clients need to reach the physical server’s subnet using the servers’ RIPs, add the following route.

       client1% route add 192.0.0.0/24 20.0.0.100

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |